**Component 4/Unit 3 - Computer hardware and architecture**

**Bibliography**

1. Computed Tomography (CT): Questions and Answers, <http://www.cancer.gov/cancertopics/factsheet/Detection/CT>, “Computed tomography (CT) is a diagnostic procedure that uses special x-ray equipment to obtain cross-sectional pictures of the body. The CT computer displays these pictures as detailed images of organs, bones, and other tissues. This procedure is also called CT scanning, computerized tomography, or computerized axial tomography (CAT).” U. S. National Institute of Health, National Cancer Institute, Online, 2010.
2. Wikipedia, “…a nuclear medicine imaging technique which produces a three-dimensional image or picture of functional processes in the body.” Online: <http://en.wikipedia.org/wiki/Positron_emission_tomography>, 2010.
3. Stephen Hawking, Wikipedia, Online: <http://en.wikipedia.org/wiki/Stephen_Hawking>. “During a visit to the research centre CERN in Geneva in 1985, Hawking contracted pneumonia, which in his condition was life-threatening as it further restricted his already limited respiratory capacity. He had an emergency tracheotomy, and as a result lost what remained of his ability to speak. He has since used an electronic voice synthesizer to communicate.” 2010.
4. ASCII, Online: <http://en.wikipedia.org/wiki/ASCII>, “ASCII includes definitions for 128 characters: 33 are non-printing control characters (now mostly obsolete) that affect how text and space is processed;[6] 94 are printable characters, and the space is considered an invisible graphic.[7] The most commonly used character encoding on the World Wide Web was US-ASCII[8] until December 2007, when it was surpassed by UTF-8.” 2010.
5. Dr. John Atanasoff (ABC computer), Online: <http://en.wikipedia.org/wiki/Atanasoff-Berry_Computer>, 2010.
6. George Boole, inventor of Boolean Logic, Online: <http://en.wikipedia.org/wiki/George_Boole>.
7. Terabytes, <http://en.wikipedia.org/wiki/Terabyte>. “The U.S. Library of Congress Web Capture team has claimed that "As of February 2010, the Library has collected almost 160 terabytes of data.”” 2010.
8. Biomedical Informatics, 3rd Edition, Shortliffe & Cimino, Springer Press, pp. 634-35. Chest X-ray consumes approx. 20 MB storage space.
9. Central Processing Unit, Online: <http://en.wikipedia.org/wiki/Central_processing_unit>, 2010.
10. Windows Embedded Web site, Online: <http://www.microsoft.com/windowsembedded/en-us/default.mspx>, 2010.
11. Wikipedia, Medical untrasonography, “Orthogonal planes of a 3 dimensional sonographic volume with transverse and coronal measurements for estimating foetal cranial volume.” Online: <http://en.wikipedia.org/wiki/Medical_ultrasonography>, 2010.
12. SonoSite, Inc., M-Turbo Portable Ultrasound, ultrasound device, Online: <http://www.microsoft.com/windowsembedded/en-us/about/casestudies/m-turbo.mspx>, 2010.
13. Intel Embedded Community, “Roving Reporter: Medical Design Part 2: The Need for Speed and endurance, by JenniferH-Osm, dated April 13, 2010, Online: <http://community.edc.intel.com/t5/Applications-Other-Blog/Roving-Reporter-Medical-Design-Part-2-The-need-for-speed-and/ba-p/2612>. “In medical imaging, a picture is worth a thousand words and several gigabytes of data. MRI and CT scans, mass-spectrometry, phenotyping, and genetic studies generate hundreds of terabytes of data that must be processed and stored by powerful supercomputers, like the [Intel Xeon-based SGI Altix UV](http://www.sgi.com/company_info/newsroom/press_releases/2010/january/icr.html) being used to support the efforts of the Institute of Cancer Research in England. Companies that manufacture medical imaging equipment rely on embedded technology vendors to deliver high-performance components that won’t break down prematurely. This type of equipment (such as the GE Healthcare CT750 HD computed tomography scanner pictured below) requires massive computing power to manipulate data and project it as Picture Archive and Communication System (PACS)-level images for radiologists to read on high-definition displays, says Clayton Tucker, senior marketing manager at Emerson Network Power Embedded Computing, a Premier member of Intel® Embedded Alliance.”